**Product Specifications.**

PoE : Passive POE (non 802.3af).

Input : 18 – 28V.

Power: 4,5 Cable Pins - 9-48V; 7,8 Pins – Return.

Max. Current : 2 A.

Ethernet Cable Length: Up to 60m.

Ethernet Speed : 10/100Mbps.