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	ELECTRICAL SPECIFICATIONS

	Model Number
	25102-1/P-5
	25102-0/P-5
	25104-1/P-5
	25104-0/P-5
	25108-1/P-5

	Frequency Band (MHz)
	300-512

	# of Channels
	2
	3-4
	5-8

	Pass Band
	3-10 MHz

	# of Resonators
	5

	Rx/Rx Isolation
	23+ dB

	System Voltage
	115 VAC

	Amplifier Gain
	+30

	Amplifier Type
	Bipolar

	Amplifier Noise Figure
	3.0 dB

	Amplifier 3rd Order IP
	+42 dBm

	Amplifier 1 dB Comp
	+21 dBm

	Amplifier Bias Voltage
	13.6 VDC

	Amplifier Current Draw
	200 mA

	System NF (typ.)
	5.0 dB

	Nominal Inpedance
	50 Ω

	Max. VSWR @ Resonance
	1.25:1

	Temperature Range
	- 22 to +140� F
-30 to +60� C

	MECHANICAL SPECIFICATIONS

	Dim (WxD)   Inches
                   Metric
	5 1/4 x 19 x 10
134 x 483 x 254

	Connectors
	N / BNC
	N / N
	N / BNC
	N / N
	N / BNC

	Ship Weight: lbs / kg.
	12 / 5.4
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	ELECTRICAL SPECIFICATIONS

	Model Number
	25108-0/P-5
	25112-1/P-5
	25112-0/P-5
	25116-1/P-5
	25116-0/P-5

	Frequency Band (MHz)
	300-512

	# of Channels
	5-8
	9-12
	13-16

	Pass Band
	3-10 MHz

	# of Resonators
	5

	Rx/Rx Isolation
	23+ dB

	System Voltage
	115 VAC

	Amplifier Gain
	+30 dB

	Amplifier Type
	Bipolar

	Amplifier Noise Figure
	3.0 dB

	Amplifier 3rd Order IP
	+42 dBm

	Amplifier 1 dB Comp
	+21 dBm

	Amplifier Bias Voltage
	13.6 VDC

	Amplifier Current Draw
	200 mA

	System NF (typ.)
	5.0 dB

	Nominal Inpedance
	50 Ω

	Max. VSWR @ Resonance
	1.25:1

	Temperature Range
	- 22 to +140� F
-30 to +60� C

	MECHANICAL SPECIFICATIONS

	Dim (WxD)   Inches
                   Metric
	5 1/4 x 19 x 10
134 x 483 x 254
	8 3/4 x 19 x 10
223 x 483 x 254

	Connectors
	N / N
	N / BNC
	N / N
	N / BNC
	N / N

	Ship Weight: lbs / kg.
	12 / 5.5
	15 / 6.9
	17 / 7.8



	



	[image: http://www.wiscointl.com/emr/multicoupler/images/251241P5.gif]
25124-1/P-5
	[image: http://www.wiscointl.com/emr/multicoupler/images/251320P5.gif]
25132-0/P-5



	



	ELECTRICAL SPECIFICATIONS

	Model Number
	25124-1/P-5
	25124-0/P-5
	25132-1/P-5
	25132-0/P-5

	Frequency Band (MHz)
	300-512

	# of Channels
	17-24
	25-32

	Pass Band
	3-10 MHz

	# of Resonators
	5

	Rx/Rx Isolation
	23+ dB

	System Voltage
	115 VAC

	Amplifier Gain
	+30 dB

	Amplifier Type
	Bipolar

	Amplifier Noise Figure
	3.0 dB

	Amplifier 3rd Order IP
	+42 dBm

	Amplifier 1 dB Comp
	+21 dBm

	Amplifier Bias Voltage
	13.6 VDC

	Amplifier Current Draw
	200 mA

	System NF (typ.)
	5.0 dB

	Nominal Inpedance
	50 Ω

	Max. VSWR @ Resonance
	1.25:1

	Temperature Range
	- 22 to +140� F
-30 to +60� C

	MECHANICAL SPECIFICATIONS

	Dim (WxD)   Inches
                   Metric
	12 1/4 x 19 x 10
312 x 483 x 254

	Connectors: Input
                  Output
	N
BNC
	N
N
	N
BNC
	N
N

	Ship Weight: lbs / kg.
	21 / 9.6
	23 / 10.5
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	ELECTRICAL SPECIFICATIONS

	Model Number
	25108-1/DP-5
	25108-0/DP-5
	25112-1/DP-5
	25112-0/DP-5
	25116-1/DP-5

	Frequency Band (MHz)
	300-512

	# of Channels
	5-8
	9-12
	13-16

	Pass Band
	3-4 MHz

	# of Resonators
	5

	Rx/Rx Isolation
	23+ dB

	System Voltage
	115 VAC

	Amplifier Gain
	+30 dB

	Amplifier Type
	Bipolar

	Amplifier Noise Figure
	3.0 dB

	Amplifier 3rd Order IP
	+42 dBm

	Amplifier 1 dB Comp
	+21 dBm

	Amplifier Bias Voltage
	13.6 VDC

	Amplifier Current Draw
	200 mA

	System NF (typ.)
	5.0 dB

	Nominal Inpedance
	50 Ω

	Max. VSWR @ Resonance
	1.25:1

	Temperature Range
	- 22 to +140� F
-30 to +60� C

	MECHANICAL SPECIFICATIONS

	Dim (WxD)   Inches
                   Metric
	8 3/4 x 19 x 10
223 x 483 x 254
	12 1/4 x 19 x 10
312 x 483 x 254

	Connectors: Input / Output
	N / BNCN
	N / N
	N / BNC
	N / N
	N / BNC

	Ship Weight: lbs / kg.
	22 / 10.0
	24 / 10.9
	26 / 11.8
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	ELECTRICAL SPECIFICATIONS

	Model Number
	25116-0/DP-5
	25124-1/DP-5
	25124-0/DP-5
	25132-1/DP-5
	25132-0/DP-5

	Frequency Band (MHz)
	300-512

	# of Channels
	5-8
	17-24
	25-32

	Pass Band
	3-4 MHz

	# of Resonators
	5

	Rx/Rx Isolation
	23+ dB

	System Voltage
	115 VAC

	Amplifier Gain
	+30 dB

	Amplifier Type
	Bipolar

	Amplifier Noise Figure
	3.0 dB

	Amplifier 3rd Order IP
	+42 dBm

	Amplifier 1 dB Comp
	+21 dBm

	Amplifier Bias Voltage
	13.6 VDC

	Amplifier Current Draw
	200 mA

	System NF (typ.)
	5.0 dB

	Nominal Inpedance
	50 Ω

	Max. VSWR @ Resonance
	1.25:1

	Temperature Range
	- 22 to +140� F
-30 to +60� C

	MECHANICAL SPECIFICATIONS

	Dim (WxD)   Inches
                   Metric
	12 1/4 x 19 x 10
312 x 483 x 254
	15 3/4 x 19 x 10
312 x 483 x 254

	Connectors: Input / Output
	N / N
	N / BNC
	N / N
	N / BNC
	N / N

	Ship Weight: lbs / kg.
	26 / 11.8
	28 / 12.8
	30 / 13.7
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