

**Pro Series**

**Industrial Router**

**UR32**


UR32 is a cost-effective industrial cellular router with embedded intelligent features that are designed for multifarious M2M/IoT applications. Global WCDMA and 4G LTE carrier supported make this drop-in connectivity a great help for operators in maximizing uptime.

Integrating embedded cellular modem and dual SIM function, the UR32 provides 3G/4G cellular network with 150 Mbps download and 50 Mbps uplink, it also has 2 fast Ethernet ports and supports Wi-Fi that compliance with 802.11b/g/n standard. All these capabilities deliver users an uninterrupted internet access.

Easy deployment and comprehensive remote device management makes UR32 versatile in most of IoT/M2M applications.



* Application Example



|  |  |  |
| --- | --- | --- |
| * Benefits * NXP industrial grade processor * Global 4G LTE CAT4/3G network with dual SIM cards for backup between multiple carrier networks * Embedded Python SDK for secondary development * Flexible modular design provides users with different connection modules like Ethernet, I/O, serial port, Wi-Fi, GPS for connecting diverse field assets * Rugged enclosure, optimized for DIN rail or shelf mounting * 3-year warranty included * Security & Reliability * Automated failover/failback between Ethernet, Cellular (dual SIM) and Wi-Fi * Secure transmission with VPN tunnels like IPsec/OpenVPN/GRE/L2TP/PPTP/DMVPN * Embeds hardware watchdog to automatically recover from various failures, ensure highest level of availability * Establishes a secured mechanism on centralized authentication and authorization of device access by supporting AAA (Radius, TACACS+, LDAP, local Authentication) and multiple levels of user authority |  | * Capabilities * Link remote devices in an environment where communication technologies are constantly changing * Support 802.11 b/g/n, as AP or client mode, to establish versatile wireless network or be the backup WAN link for 4G/3G * Support rich protocols like SNMP, Modbus bridging, RIP, OSPF * Support wide operating temperature ranging from -40°C to +70°C/-40℉ to +158℉ * Easy Maintenance * DeviceHub provides easy setup, mass configuration, and centralized management of remote devices * The user-friendly web interface design and more than one option of upgrade help administrator to manage the device as easy as pie * WEB GUI and CLI enable the admin to achieve simple management and quick configuration among a large quantity of devices * Efficiently manage the remote routers on the existing platform through the industrial standard SNMP |


* Specifications

|  |  |
| --- | --- |
| **Hardware System** | |
| CPU | ARM Cortex-A7，528 MHz |
| Memory | 128 MB DDR3 RAM and 128MB Flash |
| Extendable Storage | 1 × Micro SD |
| **Cellular Interface** | |
| Antenna Connector | 2 × 50 Ω SMA Connectors (Center PIN: SMA Female) |
| SIM Slots | 2（Mini SIM-2FF） |
| **Ethernet Interface** | |
| Numbers | 2 × 10/100 Mbps |
| Property | 1 × WAN + 1 × LAN or 2 × LAN |
| Mode | Full or half duplex (Auto-Sensing) |
| PoE | 2 × 802.3 af/at PoE PSE on LAN Ports (Optional) |
| **Wi-Fi Interface (Optional)** | |
| Antenna Connector | 1 × 50 Ω SMA Connector (Center PIN: RP-SMA Female) |
| Standards | IEEE 802.11 b/g/n，2.4GHz |
| Tx Power | 802.11b: 16 dBm +/-1.5 dBm (11 Mbps)  802.11g: 14 dBm +/-1.5 dBm (54 Mbps)  802.11n: 13 dBm +/-1.5 dBm (65 Mbps, HT20/40 MCS7) |
| Modes | AP or Client mode |
| Security | WPA/WPA2 authentication, WEP/TKIP/AES encryption |
| **GPS (Optional)** | |
| Antenna Connector | 1 × 50 Ω SMA Connector (Center PIN: SMA Female) |
| Protocol | NMEA0183, PMTK |
| **Serial Interface** | |
| Numbers | 1 × RS232 (RS485 Optional) |
| Connector | 3.5mm Terminal Block |
| Baud Rate | 300bps to 230400bps |
| **DI/DO** | |
| Numbers | 1 × DI (dry contact) + 1 × DO (wet contact), Galvanic Isolation |
| Connector | 3.5mm Terminal Block |
| Maximum V/A | 0.3A@30VDC (DO) |
| **Others** | |
| Reset Button | 1 × RESET |
| LED Indicators | 1 × POWER, 1 × SYSTEM, 1 × SIM, 3 × Signal strength |
| Built-in | Watchdog, Timer |
| **Software** | |
| Network Protocols | IPv4/IPv6, PPP, PPPoE, SNMP v1/v2c/v3, TCP, UDP, DHCP, RIPv1/v2, OSPF, DDNS, VRRP, HTTP, HTTPS, DNS, ARP, QOS, SNTP, Telnet, VLAN, SSH, etc. |
| VPN | DMVPN, IPsec, OpenVPN, PPTP, L2TP, GRE |
| Security | Access Control, DMZ, Port Mapping, MAC Binding, SPI Firewalls,  DoS&DDoS Protection, Filtering(IP&Domain), IP Passthrough |
| Management | Web, CLI, SMS, On-demand dial up, SNMP v1/v2/v3, DeviceHub |
| AAA | Radius, Tacacs+, LDAP, Local Authentication |
| Multilevel Authority | Multiple Levels of User Authority |
| Reliability | VRRP, WAN Failover, Dual SIM Backup |
| Serial Port | Transparent(TCP Client/Server, UDP), Modbus Master/Slave, Modbus Gateway (Modbus RTU to Modbus TCP) |
| **Power Supply and Consumption** | |
| Power Connector | 2-pin 5.08 mm Terminal Block |
| Input Voltage | 9-48 VDC, with Surge-Protection and Reverse Polarity Protection |
| Power Consumption | Typical 1.9 W, Max 2.4 W (In Non-PoE mode) |
| **Physical Characteristics** | |
| Ingress Protection | IP30 |
| Housing & Weight | Metal, 271 g |
| Dimension | 108 x 90 x 26 mm (4.25 x 3.54 x 1.02 in) |
| Installation | Desktop, Wall or DIN Rail Mounting |
| **Environmental** | |
| Operating Temperature | -40°C to +70°C (-40℉ to +158℉)  Reduced Cellular Performance Above 60°C |
| Storage Temperature | -40°C to +85°C (-40℉ to +185℉) |
| Ethernet Isolation | 1.5 kV RMS |
| Relative Humidity | 0% to 95% (non-condensing) at 25°C/77℉ |
| **Approvals** | |
| Regulatory | CE, FCC, RCM, NBTC, SPDDI |
| Carrier | PTCRB, AT&T |
| Environmental | RoHS |
| EMC | EN 55032, EN 55035 |
| EMS | IEC 61000-4-2 Level 3  IEC 61000-4-3 Level 2  IEC 61000-4-4 Level 2  IEC 61000-4-5 Level 2  IEC 61000-4-6 Level 3  IEC 61000-4-8 Level 1  IEC 61000-4-11 Level 3 |
| Radio Frequency | EN 301 489-1/17/19/52, EN 301 511, EN 301 908-1/2/13, EN 303 413, EN300 328 |
| Safety | EN62368-1 |

* Dimensions(mm)
* Accessories




2 × Magnetic Cellular Antennas

****



4 × Wall Mounting Kits




1 × DIN Rail Kit



1 × 6-Pin Pluggable

Terminal



1 × Power Adapter



1 × Wi-Fi Antenna

**(Wi-Fi Version Only)**



2 × Stubby Cellular Antennas **(Optional)**



1 × GPS Antenna

**(GPS Version Only)**

**\*Note:** Contact us if you need any other special accessories or customized accessories.